Feng Chia University

Electrical Engineering Fundamentals I Lab

Laboratory 9

Diodes V-I Characteristics

Instructor: Prof. Shyan-Lung Lin

Student Name: 周嘉禾

Student ID: D1166506

Experiment Date:14/12/2023

1. Introduction
2. To apply the forward and reverse bias to a diode
3. To understand the voltage current characteristics of a diode
4. Materials
   1. DC Power Supply
   2. Digital multimeter
   3. Devices
      1. Variable Resistor RT 10 kΩ (B) ×1
      2. Resistors: R = 1 kΩ ×1
      3. Diode: D 1N4001 ×1
5. Circuit diagram

一張含有 文字, 螢幕擷取畫面, 圖表, 字型 的圖片

自動產生的描述

▲ Figure 1. Circuit of Experiment 9.a Forward Bias Measurement

一張含有 文字, 圖表, 螢幕擷取畫面, 字型 的圖片

自動產生的描述

▲ Figure 2. Circuit of Experiment 9.b Reverse Bias Measurement

1. Methods

Use digital multimeter to measure voltage and current across the diode.

1. Experiments data
   1. Experiment 9.a

Table 1: Results of forward bias measurement across the diode

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Forward Bias | 0 V | 0.1 V | 0.2 V | 0.3 V |
| Forward Current | 0.3 μA | 0.4 μA | 0.6 μA | 1.8 μA |

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Forward Bias | 0.4 V | 0.5 V | 0.6 V | 0.6201 V |
| Forward Current | 19.2 μA | 189.1 μA | 1366.3 μA | 2000 μA |

* 1. Experiment 9.b

Table 2: Results of reverse bias measurement across the diode

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Reverse Bias | 0 V | 0.5 V | 1 V | 2 V |
| Reverse Current | 0.3 μA | 0.4 μA | 0.4 μA | 0.4 μA |

|  |  |  |  |
| --- | --- | --- | --- |
| Reverse Bias | 3 V | 4 V | 5 V |
| Reverse Current | 0.4 μA | 0.5 μA | 0.6 μA |

1. Results

None

1. Discussion

It’s hard to adjust variable resistor, a little bit of move will cause tremendous changes. Nevertheless, sometimes, the variable resistor can’t let the voltage be zero, it might be replaced by greater variable resistor in order to approach zero voltage.

1. Conclusion

By measuring voltage and current across the diode, it’s easy to determine either forward bias or reverse bias.